|  |
| --- |
| **Product Detail** |
| Ports | 　16GE POE+2SFP | Switch Capacity | 　56Gbps |
| Switch Chip | 　RTL8382L | Forwarding Rate | 　40.32Mpps |
| Packet Buffer | 　4.1M | Flash Memory | 　8M |
| DDRIII Capacity | 　-- | Stackability | 　NO |
| MAC Address Table | 　8K | Input Power | 100～240V 50-60Hz |
| Jumbo Frames | 　9k | Max Power Consumption | 　350w |
| VLAN | 　Ports isolation | Warranty | 　1 |

|  |  |
| --- | --- |
| **Title** | **16 ports 10/100/1000Mbps POE switch** |
| **Price** | **104.5USD** |
| **Feature** | **Ports isolation one key setting** |
| **Model**  | **18u16G16Ph2S-350I** |

|  |  |
| --- | --- |
| Fixed Port | 16\*10/100/1000Base-TX PoE port（Data/Power） 2\*1000M SFP |
| PoE Ports | 1-16 port supports PoE  |
| Function | N:(Standard normal)V:(Port isolation)S:(Super mode) |
| Network Protocol | IEEE 802.3 IEEE 802.3i 10BASE-TIEEE 802.3u 100BASE-TXIEEE 802.3ab1000BASE-T IEEE 802.3x IEEE 802.3z 1000BASE-XIEEE 802.3af/at  |
| PoE Standard | IEEE802.3af/at |
| Port Specification | 10/100BaseT（X）Auto |
| Transmission Mode | Store and Forward(full wirespeed) |
| Bandwidth  | 56Gbps  |
| Packet Forwarding  | 40.32Mpps |
| MAC Address | 8K |
| Buffer  | 4.1M |
| Transmission Distance | 10BASE-T ： Cat3,4,5 UTP(≤250 meter) 100BASE-TX ： Cat5 or later UTP(150 meter) 1000BASE-TX ： Cat6 or later UTP(150 meter)1000BASE-SX:62.5μm/50μm MMF(2m~550m)1000BASE-LX:62.5μm/50μm MM(2m~550m) or 10μm SMF(2m~5000m) |
| Power Pin | Default 1/2(+)，3/6(-)；Optional order4/5(+)，7/8(-) |
| Single port power | Average 15.4W；MAX 30W  |
| Total power/Input voltage | MAX 350W （AC100-240V 50/60HZ） |
| Watt  | Standby Power Consumption：≤20W； |
| LED Indicator | PWR:Power LED1-16:(Link LED=10/100M Link、1000M=Gigabit Link)17 18:(SFP LED) |
| Power Input | Built-in power AC：100～240V 50-60Hz 1A |
| Operating Temperature/Humidity | -10～+55°C；5%～90% RH Non coagulation |
| Storage Temperature/Humidity | -40～+75°C；5%～95% RH Non coagulation |
| Product size/Packingsize（L\*W\*H） | 440mm\*290mm\*45mm515mm\*375mm\*95mm |
| N.W/G.W（kg） | 3.2kg/3.9kg |
| Installation | Rack-mount(optional machine hanger spare parts) |
| Lightning protection level  | 3KV 8/20us；IP30 |
| Certificate  | CE mark, commercial；CE/LVD EN60950；FCC Part 15 Class B；RoHS； |
| Warranty  | Whole device for 1 year（full wirespeed） |